


# BTH






没有write response，有read response


## Send only




### UD send only




## Send middle




## Send last




## Send first







## acknowledge



## Write only




### Write only2




## Read

### Read request




### Read reponse




# RETH


VA(8B)：表明数据包要存放的虚拟起始地址  
r\_key(4B)：表明该虚拟地址的访问权限  
dma length(4B)：该包的长度

## Rdma write first







## Rdma request




# AETH




## ack



## Read reponse





# Send only with invalidate

